RadioLink T8S Radio Transmitter/Receiver Setup
-----------------------------------------------

Driver Installation:

	Open the CH340_Driver folder
	Run the DRVSETUP64 application (You will have to allow the app to make changes to your device)
	Make sure CH31SER.INF is selected from the drop-down menu at the top of the setup app
	Press the INSTALL button
	The drivers will be successfully installed in a few moments (a pop-up will confirm successful installation)


Transmitter Configuration Setup:
	
	Plug your T8S transmitter into your computer using the provided USB cable (or any other USB-A to microUSB cable)
	Press and hold the center button on the transmitter until it beeps and green lights above the button turn on
	Open the Radiolink_parameter_setting_software_V4.2 folder
	The software requires no installation, run the Radiolink_parameter_settings application
	In the drop-down menu next to the large OPEN button at the top of the program, select the correct transmitter port
		The port will be named COM followed by a number (the number will vary from computer to computer)
	Press the OPEN button, your transmitter should begin to beep
	On the transmitter, press any one of the subtrim buttons (the small buttons with arrows on them)
	The beeping will stop, and your transmitter will be connected to the configuration program
	Confirm your transmitter is connected by moving one of the sticks on the transmitter, you should see the program change


Switching From Mixed Configuration to Tank Configuration:
	Connect your transmitter to the provided configuration software (see above)
	Press the large LOAD button at the top of the program
	A file-select window will pop-up, open the folder named "configurations"
	Select the file named t8s_tank and press open
	Press the large WRITE button at the top of the program, your transmitter will beep 3 times
	Your transmitter is now in the Tank Configuration
	
	To switch back to the original mixed configuration, repeat above steps except select the file named t8s_mixed
